Calculations:

Vth /(Rth+Rl ) = Current Through Load

Observation: <[Observation]>

Calculated Value: <[Current]>

<[Observation]> = <[Current]>

Calculated value matches our observation, hence the theorem is correct.

For powersupply label

<link href="http://fonts.cdnfonts.com/css/seven-segment" rel="stylesheet">

.PSdisplay {

    position: relative;

    background-color: rgba(24, 22, 22, 0.834);

    color: red;

    text-align: center;

    font-family: 'Seven Segment';

    font-weight: bold;

    border: inset;

    font-size: 40px;

    width: 80px;

    height: 40px;

    right: 11em;

    top: 2em;

}